**Holley HP Universal and Accufab Throttle Bodies**

The IAC on the Accufab throttle bodies is the later GM style. This is good, but you will have to swap two wires on the Holley IAC connector harness.

Swap positions A & C: the **purple blue** & **purple white** wires.

There are two ways to do this:

1) Strip back the covering and cut and swap the wires using solder and heat shrink. The wires are very small so the covering will cover everything.

2) Swap the pins. It’s very easy and here’s a link to a video:

<https://www.youtube.com/watch?v=6dfigDyUUw4&feature=youtu.be>